ZQZ5041TQZQ6型清障车 (Tow Truck) Technical Specifications
	Parameter
	Value

	Model
	ZQZ5041TQZQ6型清障车 (Tow Truck)

	Dimensions
	5995x2380x2330/2280x2200 mm

	Total Weight
	4495 kg

	Curb Weight
	2865 kg

	Passenger Capacity
	Not specified

	Chassis Model
	QL1040MVHAY

	Manufacturer
	Qingling Motors Co., Ltd.

	Axle Number
	Not specified

	Wheelbase
	3360 mm, 3600 mm, 2800 mm

	Tire Number & Specs
	7.00R16LT 8PR, 6.50R16LT 10PR, 7.00R16LT

	Fuel Type
	Diesel

	Emission Standard
	GB17691-2018 National VI

	Engine Model
	4KK1N6LB, 4KK1N6SD, 4KB1-TCG60

	Engine Power
	120, 132, 130 HP

	Engine Displacement
	2498 cc, 2499 cc

	Top Speed
	115 km/h (with 4KB1-TCG60 engine)

	Special Features
	Flatbed and winch, no towing function, optional flip or integrated board styles, two side operation boxes, ABS, and air/hydraulic brake systems.

	Side Protection Material
	Q235, Bolt connection

	Rear Protection
	Q235, Welded connection, dimensions: 100x50 mm, ground clearance: 490 mm

	Maximum Load on Flatbed
	1500 kg






